**Overview**

**Quick Details**

Place of Origin:

Jiangsu, China (Mainland)

Brand Name:

MANORSHI

Model Number:

MSO-PT1040H07R

Usage:

Level Sensor

Theory:

Ultrasonic Sensor

Output:

Digital Sensor

Product Name:

Ultrasonic Sensor

Construction:

open type

Using method:

transmitter or receiver

Color:

black

center frequency:

40kHz

Dimension:

10mm

Price:

cheap

Performance:

good

Housing Material:

ABS

SPL:

≥110dB

**Supply Ability**

Supply Ability:

5000 Piece/Pieces per Day for 40kHz Ultrasonic Sensor

**Packaging & Delivery**

Packaging Details

Standard Export package for 40kHz Ultrasonic Sensor

Port

China Port for 40kHz Ultrasonic Sensor

Lead Time :

|  |  |  |
| --- | --- | --- |
| Quantity(Pieces) | 1 - 1000 | >1000 |
| Est. Time(day) | 4 | To be negotiated |

Product Description

|  |  |  |
| --- | --- | --- |
| **Item** | **Transmitter** | Receiver |
| **Center frequency** | 40.0±1.0KHz | |
| **SPL** | ≥110dB | ------- |
| **Sensitivity** | ------- | ≥-67dB |
| **Directivity** | 60°±15° | |
| **Capacitance** | 2300±30%pF | |
| **Housing material** | Aluminum Or Plastic | |
| **Measure distance** | 0.2～18m | |
| **Driving Voltage** | ≤40Vrms | |
| **Operating Temperature** | -20～+70℃ | |
| **Storage Temperature** | -40～+85℃ | |

